GE Method to Reduce FCI in LWR’s - After Adamson

Oxide Fuel

Zr-2 or Zr-4 Cladding

500-1,000m thick

Zr Sponge Liner (Bonded)

< 1,000 wt ppm impurities

25-100 m thick

(Bonded)

Implanted Layer

0-0.5% Cr, Fe, N, Cu

0.01 to 1

Patent # 4,894,203