The Reasons for DevelopingLow Activation Stainless SteelsHave Not Always Been the Same

WasteDisposal

Safety

Maintenance

Recycling

Near SurfaceBurial (Class C)

<10 RemMaximum EarlyDose

< 1 mrem/hrContact Dose

Contact Dose

< 1 rem/hr , t<100 Y< 1 mrem/hr, t>100 Y